SPI FlashROM Programmer 2.14 by RayeR
*************************************

SPIPGM	    - binary for Linux
SPIPGM.EXE  - binary for DOS/Win9x
SPIPGMW.EXE - binary for Win9x/NT/2k/XP
IOPERM.DLL  - low-level HW access library for Win9x/NT/2k/XP/Vista/7(NoUAC)

Version 1.7+ has improved LPT port handling resulting in 1,6x faster reading

Version 2.0 +extended FlashROM identification (some old non-JEDEC ID chips)
	    +support for AAI Byte/Word programming modes (some SST FlashROMs)
	    +verify command (compare FlashROM content against file)
	    +block erase command (some ST FlashROMs)
	    +allow images smaller than FlashROM size (displays warning)
	    +read speed up +25%
	    +write speed up +41%

SPI FlashROMs supported (new are marked with *)
***********************************************

AMIC:
A25L05PU/PT (64kB)
A25L10PU/PT (128kB)
A25L20PU/PT (256kB)
A25L40PU/PT (512kB)
A25L80PU/PT (1MB)
A25L16PU/PT (2MB)
A25L32PU/PT (4MB)
A25L64PU/PT (8MB)
A25L512 (64kB)
A25L010 (128kB)
A25L020 (256kB)
A25L040 (512kB)
A25L080 (1MB) - tested OK

Atmel:
AT25F512B (64kB)
AT25DF021 (256kB)
AT26DF041 (512kB)
AT25DF041A (512kB)
AT26F004 (512kB) - tested OK
AT26DF081 (1MB)
AT25/26DF081A (1MB)
AT25DF081 (1MB)
AT26DF161 (1MB)
AT26DF161A (2MB)
AT25DF161 (2MB)
AT25DQ161 (2MB)
AT25/26DF321 (4MB)
AT25DF321A (4MB)
AT25DQ321A (4MB)
AT25DF641(A) (8MB)

EON:
EN25B10 (128kB)
EN25B20 (256kB)
EN25B40(T) (512kB)
EN25B80 (1MB)
EN25B16 (2MB)
EN25P32 (4MB)
EN25P64 (8MB)
EN25P128 (16MB)
EN25Q40 (512kB)
EN25Q80 (1MB)
EN25Q16 (2MB)
EN25Q32 (4MB)
EN25Q64 (8MB)
EN25Q128 (16MB)
EN25F10 (128kB)
EN25F20 (256kB)
EN25F40 (512kB)
EN25F80 (1MB) - tested OK
EN25F16 (2MB)
EN25F32 (4MB)
EN25F64 (8MB)
EN25F128 (16MB)

ESMT:
F25L004A (512kB) - tested OK
F25L008A/08PA (1MB)
F25L016A/16PA (2MB)
F25L32PA (4MB)
F25L64PA (8MB)
F25S04PA (512kB)
F25L08PA (1MB)
F25L016QA (2MB)
F25L32QA (4MB)
F25L64QA (8MB)

GigaDevice:
GD25Q512 (64kB)
GD25Q10 (128kB)
GD25Q20 (256kB)
GD25Q40 (512kB)
GD25Q80 (1MB)
GD25Q16 (2MB) - tested OK
GD25Q32 (4MB)
GD25Q64 (8MB)

Intel:
QB25F016S33B8 (2MB)
QB25F032S33B8 (4MB)
QB25F064S33B8 (8MB)

Macronix:
MX25L512E (64kB)
MX25L1005/1006E (128kB) - tested OK
MX25L2005/2006E (256kB)
MX25L4005/4006E (512kB)
MX25L8005/8006E (1MB) - tested OK
MX25L1605/1606E (2MB) - tested OK
MX25L3205/3206E (4MB)
MX25L6405/6406E (8MB)
MX25L12835E/12836E (16MB)
MX25L25635E/25735E/25835E (32MB)

PMC:
*Pm25LD512 (64kB) - tested OK
*Pm25LD010 (128kB)
*Pm25LD020 (256kB)
Pm25LV512(A) (64kB) - tested OK
Pm25LV010(AB) (128kB)
Pm25LV020 (256kB)
Pm25LV040 (512kB) - tested OK
Pm25LV080B (1MB)
Pm25LV016B (2MB)
Pm25LV032B (4MB)
Pm25LV064B (8MB)

Spansion:
S25FL001A (128kB)
S25FL002A (256kB)
S25FL004A (512kB)
S25FL008A (1MB)
S25FL016A (2MB)
S25FL032A/P (4MB) - tested OK
S25FL064A/P (8MB)
S25FL128P/S/129P/S (16MB) - tested OK
S25FL256S (32MB)
S25FL512S (64MB)
S25FL01GS (128MB)

ST Microelectronic/Numonyx:
M25P05 (64kB)
M25P10 (128kB)
M25P10AV (128kB) - tested OK
M25P20 (256kB)
M25P40 (512kB)
M25P80 (1MB)
M25P16 (2MB)
M25P32 (4MB) - tested OK
M25P64 (8MB)
M25P128 (16MB)
M45PE10 (128kB)
M45PE20 (256kB)
M45PE40 (512kB)
M45PE80 (1MB)
M45PE16 (2MB)
M25PX80 (1MB)
M25PX16 (2MB)
M25PX32 (4MB)
M25PX64 (8MB)
N25Q032A13E (4MB)
N25Q032A11E (4MB)
N25Q064A13E (8MB)
N25Q064A11E (8MB)
N25Q128A13E (16MB)
N25Q128A11E (16MB)
N25Q256A13E (32MB)
N25Q256A11E (32MB)
N25Q512A13G (64MB)
N25Q512A11G (64MB)
N25Q00AA13GB (128MB)

SST:
SST25VF512(B) (64kB) - tested OK
SST25VF010(B) (128kB)
SST25VF020(B) (256kB)
SST25VF040(B) (512kB)
SST25VF080(B) (1MB) - tested OK
SST25VF016(B) (2MB) - tested OK
SST25VF032(B) (4MB)
SST25VF064C (8MB)
SST25VF128(B) (16MB)
SST26VF016 (2MB)
SST26VF032 (4MB)
SST26VF064 (8MB)

Winbond:
W25Q10B (128kB)
W25Q20BV (256kB)
W25Q40BV (512kB)
W25Q80BV (1MB) - tested OK
W25Q16BV (2MB) - tested OK
W25Q32BV (4MB) - tested OK
W25Q64BV (8MB)
W25Q128BV (16MB)
W25Q256FV (32MB)
W25X10 (128kB)
W25X20 (256kB)
W25X40 (512kB)
W25X80 (1MB) - tested OK
W25X16 (2MB)
W25X32 (4MB) - tested OK
W25X64 (8MB)
